# SSDTTime · GitBook

> Last modified: Thu Jun 18 2020 03:09:33 GMT+0000 (Coordinated Universal Time)

# Fixing Embedded Controllers: SSDTTime

The second involves using SSDTTime which automates most of the process. See here on how to use it: SSDTs: Easy Way

To get the SSDT-PLUG, run the following:

- `4. Dump DSDT` then run `2. FakeEC`

This will provide you with some files, the main one you care about is SSDT-EC.aml. The DSDT and .dsl are only left for referencing or verification.

The main things to note with this method:

- Doesn't work on HEDT and server hardware(ie. X99 and X299)
  - While the majority following this guide are likely on consumer hardware, those with fancier hardware will need to either use the Prebuilt or Manual method
- Doesn't work on Laptops
  - Just like with HEDT, you will need to either use the Prebuilt or Manual method
- Doesn't provide you the USBX property to fix power
  - This can easily be fixed by using this prebuilt file in addition to SSDT-EC: SSDT-USBX.aml
  - Note USBX is only needed for Skylake and newer
- Doesn't really teach you anything
  - For most, this doesn't matter. But to some knowing what makes your hackintosh tick is part of the journey

## Wrapping up

Once you're done making your SSDT, either head to the next page to finish the rest of the SSDTs or head here if you're ready to warp up:

- Cleanup

# results matching ""

# No results matching ""