# What SSDTs do each platform need | Getting Started With ACPI

# # What SSDTs do each platform need

Please see the specific ACPI section of your config.plist, all SSDTs needed are covered there with a brief explainer. But here's a very quick TL;DR:

- What SSDTs do each platform need
  - Desktop
  - High End Desktop
  - Laptop
- SSDT Creation

## # Desktop

Platforms | CPU | EC | AWAC | NVRAM | USB
--- | --- | --- | --- | --- | ---
Penryn | N/A | SSDT-EC | N/A | N/A | N/A
Lynnfield and Clarkdale
SandyBridge | CPU-PM (opens new window) (Run in Post-Install)
Ivy Bridge
Haswell | SSDT-PLUG
Broadwell
Skylake | SSDT-EC-USBX
Kaby Lake
Coffee Lake | SSDT-AWAC | SSDT-PMC
Comet Lake | N/A | SSDT-RHUB
AMD (15/16h) | N/A | N/A | N/A
AMD (17h) | SSDT-CPUR for B550 and A520 (opens new window) | N/A | N/A

## # High End Desktop

Platforms | CPU | EC | RTC | PCI
--- | --- | --- | --- | ---
Nehalem and Westmere | N/A | SSDT-EC | N/A | N/A
Ivy Bridge-E | SSDT-PLUG | SSDT-UNC
Haswell-E | SSDT-EC-USBX | SSDT-RTC0-RANGE
Broadwell-E
Skylake-X | N/A

## # Laptop

Platforms | CPU | EC | Backlight | I2C Trackpad | AWAC | USB | IRQ
--- | --- | --- | --- | --- | --- | --- | ---
Clarksfield and Arrandale | N/A | SSDT-EC | SSDT-PNLF | N/A | N/A | N/A | IRQ SSDT
SandyBridge | CPU-PM (opens new window) (Run in Post-Install)
Ivy Bridge
Haswell | SSDT-PLUG | SSDT-GPI0
Broadwell
Skylake | SSDT-EC-USBX | N/A
Kaby Lake
Coffee Lake (8th Gen) and Whiskey Lake | SSDT-PNLF-CFL
Coffee Lake (9th Gen) | SSDT-AWAC
Comet Lake
Ice Lake | SSDT-RHUB

Continuing:

Platforms | NVRAM | IMEI
--- | --- | ---
Clarksfield and Arrandale | N/A | N/A
Sandy Bridge | SSDT-IMEI
Ivy Bridge
Haswell | N/A
Broadwell
Skylake
Kaby Lake
Coffee Lake (8th Gen) and Whiskey Lake
Coffee Lake (9th Gen) | SSDT-PMC
Comet Lake | N/A
Ice Lake

## # SSDT Creation