# Fixing System Clocks (SSDT-AWAC/RTC0) | Getting Started With ACPI

# # Fixing System Clocks (SSDT-AWAC/RTC0)

- Reminder: Does not support HEDT(ie. X99 and X299)

The second involves using SSDTTime which automates most of the process. See here on how to use it: SSDTs: Easy Way

To get the SSDT-PMC, run the following:

- `7. Dump DSDT` then run `6. AWAC`

This will provide you with some files, the main one you care about is SSDT-AWAC.aml. or SSDT-RTC0.aml. The DSDT and .dsl are only left for referencing or verification.

The main things to note with this method:

- Doesn't really teach you anything
  - For most, this doesn't matter. But to some knowing what makes your hackintosh tick is part of the journey

## # Wrapping up

Once you're done making your SSDT, either head to the next page to finish the rest of the SSDTs or head here if you're ready to wrap up:

- Cleanup