# Prebuilt · GitBook

> Last modified: Thu Jun 18 2020 03:09:33 GMT+0000 (Coordinated Universal Time)

# Fixing Embedded Controllers: Prebuilt

By far the easiest way to fix your Embedded Controller is just downloading one of the files below:

Desktop:

- SSDT-EC-USBX-DESKTOP
  - For Skylake desktops and newer and AMD CPU based systems
- SSDT-EC-DESKTOP
  - For Broadwell desktops and older

Laptops:

- SSDT-EC-USBX-LAPTOP.aml
  - For Skylake laptops and newer
- SSDT-EC-LAPTOP.aml
  - For Broadwell laptops and older

The main things to note with this method:

- Quite Bloated
  - There's ACPI naming for every type, this means there's added delays in boot times
- Doesn't really teach you anything
  - For most, this doesn't matter. But to some knowing what makes your hackintosh tick is part of the journey

## Wrapping up

Once you're done making your SSDT, either head to the next page to finish the rest of the SSDTs or head here if you're ready to warp up:

- Cleanup

# results matching ""

# No results matching ""