# Choosing the SSDTs · GitBook

> Last modified: Thu Jun 18 2020 03:09:34 GMT+0000 (Coordinated Universal Time)

# What SSDTs do each platform need

Please see the specific ACPI section of your config.plist, all SSDTs needed are covered there with a brief explainer. But here's a very quick TL;DR:

- What SSDTs do each platform need
  - Desktop
  - Laptop
  - SSDT Creation

## Desktop

Platforms | CPU | EC | AWAC | NVRAM | USB
--- | --- | --- | --- | --- | ---
Ivy Bridge | CPU-PM (Run in Post-Install) | SSDT-EC | N/A | N/A | N/A
Ivy Bridge-E
Haswell/Broadwell | SSDT-PLUG
Haswell-E
Broadwell-E
Skylake | SSDT-EC-USBX
Skylake-X
Kabylake
CoffeeLake | [SSDT-AWAC]/Universal/awac.html) | SSDT-PMC
CometLake | SSDT-RHUB
AMD (15/16/17h) | N/A | N/A | N/A | N/A

## Laptop

Platforms | CPU | EC | Backlight | I2C Trackpad | AWAC | USB | IRQ
--- | --- | --- | --- | --- | --- | --- | ---
Ivy Bridge | CPU-PM (Run in Post-Install) | SSDT-EC | SSDT-PNLF | SSDT-GPI0 | N/A | N/A | IRQ SSDT
Haswell | SSDT-PLUG
Broadwell
Skylake | SSDT-EC-USBX | N/A
KabyLake
CoffeeLake (8th Gen) | SSDT-PNLF-CFL
CoffeeLake (9th Gen) | SSDT-AWAC
CometLake
IceLake | SSDT-RHUB

## SSDT Creation

# results matching ""

# No results matching ""